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Ref. No. 09/SPAV/R&M/2026–27                                                                         Date: 18.08.2026
 NOTICE INVITING QUOTATIONS
The School of Planning and Architecture, Vijayawada, invites sealed quotations from eligible State/Central Government empaneled contractors/GST-registered agencies for the following work as per the details given below:

Name of Work: Providing and fixing powder-coated aluminum partitions with laminated particle board including pre-laminated cement-bonded boards, and supply & installation of AC units in the existing Art Lab at Academic Block, SPAV Campus, ITI Road, Vijayawada

SCHEDULE OF QUANTITIES

	S.No.
	DESCRIPTION OF ITEM
	UNIT
	QUANTITY
	AMOUNT

	1
	Providing and fixing aluminium work for doors, windows, ventilators and partitions with extruded built-up standard tubular sections/ appropriate Z sections and other sections of approved make conforming to IS: 733 and IS:1285, fixing with dash fasteners of required dia and size, including necessary filling up the gaps at junctions, i.e. at top, bottom and sides with required EPDM rubber/ neoprene gasket etc. Aluminium sections shall be smooth, rust-free, straight, mitred and jointed mechanically wherever required, including cleat angle, Aluminium snap beading for glazing/panelling, C. All the sections shall be painted with powder coating, complete all as directed by SPAV authorities. brass / stainless steel screws, all complete as per architectural drawings and the directions of the Engineer-in-charge. (Glazing, panelling, and dash fasteners to be paid for separately)
	KG
	65
	

	2
	Providing and fixing glazing in aluminium doors, windows, ventilator shutters, and partitions etc., with EPDM rubber/neoprene gasket, etc., complete as per the architectural drawings and the directions of the engineer-in-charge. (Cost of aluminium snap beading shall be paid in the basic item)
	
	
	


	a.
	With float glass panes of 4.0 mm thickness (weight not less than 10kg/sqm)
	Sqm
	04
	

	3.
	Providing and fixing 12 mm-thick pre-laminated particle board (including pre-laminated cement-bonded boards such as Bison Lam) for panelling in aluminium partitions.
	Sqm
	30
	

	4.
	Providing and fixing a Brass 100mm mortice latch and lock with 6 levers, without a pair of handles (best make of approved quality), for aluminium doors, including necessary cutting and making good, etc., complete. (with 3 nos key)
	Nos
	2
	

	5.
	Providing and fixing aluminium handles, ISI marked, anodised (anodic coating not less than grade AC 100 as per IS : 1868, transparent or dyed to the required colour or shade, with necessary screws,
etc, complete all as directed by SPAV Authorities(125 mm long length)
	Nos
	4
	

	6.
	Providing and fixing of Hydraulic door closers, Dorma/Dorset or equivalent
	Nos
	2
	

	7.
	Providing and fixing a 150 mm bright-finished floor Aluminium door stopper with a rubber cushion, complete
	Nos
	2
	

	8.
	Dismantling aluminium/ Gypsum partitions, doors, windows, fixed glazing, and false ceiling, including disposal of unserviceable material and stacking of serviceable material within 50 meters lead as directed by the Engineer-in-charge
	Sqm
	10
	

	9.
	Providing and fixing false ceiling with GI framework and 12.5 mm thick moisture-resistant gypsum board, including jointing, finishing with primer, cut-outs for fixtures, complete but excluding painting.
	Sqm
	10
	

	10.
	Wall painting with acrylic emulsion paint, having VOC (Volatile Organic Compound) content less than 50 grams/ litre, of approved brand and manufacturer, including applying additional coats wherever required, to achieve even shade and colour.
	Sqm
	10
	

	11.
	Providing and applying white cement-based putty of average thickness 1 mm, of approved brand and manufacturer, over the plastered wall surface to prepare the surface even and smooth; complete all as directed by SPAV authorities
	Sqm
	10
	

	12.
	Supply and installation of 2 Nos. 2.0 Ton, 5-Star rated AC units including installation, drainage, civil works, and other allied works.
	Nos
	02
	

	 
	Total Amount (Including all taxes)
	

	 
	Note: All the materials should comply with CPWD Specifications and ISO norms

	
	Material Specifications

	a.
	Aluminium sections: Tata/Jindal

	b.
	Door closers: Doorma /Door set

	c.
	Glazing: Toughened glass- Saint-Gobain

	d.
	Lock Sets: Godrej

	e.
	False ceiling: Gypsum 

	   f.
	Ac makes-Blue star, carrier etc-as per CPWD-approved makes




The Sealed quotations are to be submitted up to 15:00 Hrs. on or before 25.08.2026. The quotations will be opened on the same day at 15:30 hrs. The NIQ, along with the terms and conditions, can be obtained from our website, in the tender section, at www.spav.ac.in.

Terms & Conditions:
1. The sealed covers should be superscribed with the name of the work and the address of the agency quoting rates, addressed to "The Registrar, School of Planning and Architecture, Vijayawada."
2. Blank NIQ documents for quoting rates can be downloaded from the Institute website: https://www.spav.ac.in/Tenders.
3. The work should be initiated and completed by the vendor within 20 (Twenty) days from the issue of the work order
4. Specifications for the work to be carried out as per the BOQ and CPWD norms.
5. Rates shall be inclusive of all applicable taxes, expenses, and responsibilities as stated above, and no extra payments will be made.
6. No advance payment shall be made
7. Sealed quotations must be submitted with a covering letter (neatly typed) on the contractor’s letterhead.
8. The contractor should clearly mention the name of the work, the address of the agency, PAN, and GST Number on their letterhead.
9. The competent authority reserves the right to accept or reject the whole or part of the quotations.





Contractor Sign with Name & Address
------------------------------------------------------------------------------------------------
Survey No.4/4, ITI Road, Vijayawada – 520 008., A.P., India.
Email: registrar@spav.ac.in Ph: 0866- 2469446 Website: www.spav.ac.in
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